# Attaching adapter and connecting vacuum on tools with external vacuum

Required tools: Assembly tool 4080 1457 03 (for I06) or 4080 1457 02 (for HM4).

To attach the adapter and connect to the vacuum system, perform the following steps:

1. Unscrew the front protection.

2. Pull the telescope downwards to disconnect the telescope.

3. Attach the vacuum adapter holder. Use the assembly tool.

4. Adjust the placement of the vacuum adapter holder.

5. Insert the vacuum hose.

6. Attach the telescope to the vacuum adapter holder.

## Applies to: