# Collet

Ordering No. | Remark
--- | ---
4141 0677 03 | ØD 22.9 mm. Order together with 4141 0676 03.
4141 0677 04 | ØD 25.2 mm. Order together with 4141 0676 04.
4141 0814 08 | ØD 28.58 mm (1 1/8"). Order together with 4141 0810 03. Suitable for concentric collet HD.
4141 0814 16 | ØD 31.75 mm (1 1/4"). Order together with 4141 0810 04. Suitable for concentric collet HD.
4141 0814 24 | ØD 34.93 mm (1 3/8"). Order together with 4141 0810 05. Suitable for concentric collet HD.
4141 0813 01 | ØD 12.7 mm. Order together with 4141 0806 01 or 4141 0807 01 or 4141 0676 01. Suitable for concentric collet MINI and REGULAR.
4141 0813 02 | ØD 15.09 mm. Order together with 4141 0676 02. Suitable for concentric collet MINI and REGULAR.
4141 0813 03 | ØD 15.87 mm (5/8"). Order together with 4141 0806 03 or 4141 0807 03 or 4141 0676 06 or 4141 0860 03. Suitable for concentric collet MINI and REGULAR.
4141 0813 05 | ØD 16.7 mm. Order together with 4141 0806 05. Suitable for concentric collet MINI and REGULAR.
4141 0813 06 | ØD 17 mm. Order together with 4141 0806 05. Suitable for concentric collet MINI and REGULAR.
4141 0813 08 | ØD 17.7 mm. Order together with 4141 0806 08. Suitable for concentric collet MINI and REGULAR.
4141 0813 09 | ØD 18.05 mm. Order together with 4141 0806 09. Suitable for concentric collet MINI and REGULAR.
4141 0813 10 | ØD 18.4 mm. Order together with 4141 0806 10. Suitable for concentric collet MINI and REGULAR.
4141 0813 11 | ØD 18.75 mm. Order together with 4141 0806 11. Suitable for concentric collet MINI and REGULAR.
4141 0813 12 | ØD 19.05 mm (3/4"). Order together with 4141 0806 12. Suitable for concentric collet MINI and REGULAR.
4141 0813 13 | ØD 19.4 mm. Order together with 4141 0806 13. Suitable for concentric collet MINI and REGULAR.
4141 0813 14 | ØD 19.8 mm. Order together with 4141 0806 14. Suitable for concentric collet MINI and REGULAR.
4141 0813 15 | ØD 20.2 mm. Order together with 4141 0806 15. Suitable for concentric collet MINI and REGULAR.
4141 0813 16 | ØD 20.6 mm. Order together with 4141 0806 16. Suitable for concentric collet MINI and REGULAR.
4141 0813 18 | ØD 21.4 mm. Order together with 4141 0806 18. Suitable for concentric collet MINI and REGULAR.
4141 0813 20 | ØD 22.22 mm (7/8"). Order together with 4141 0806 20. Suitable for concentric collet MINI and REGULAR.
4141 0813 21 | ØD 22.6 mm. Order together with 4141 0806 21. Suitable for concentric collet MINI and REGULAR.
4141 0813 22 | ØD 23 mm. Order together with 4141 0806 22. Suitable for concentric collet MINI and REGULAR.
4141 0813 23 | ØD 23.4 mm. Order together with 4141 0806 23. Suitable for concentric collet MINI and REGULAR.
4141 0813 24 | ØD 23.8 mm. Order together with 4141 0806 24. Suitable for concentric collet MINI and REGULAR.
4141 0813 26 | ØD 24.6 mm. Order together with 4141 0806 26. Suitable for concentric collet MINI and REGULAR.
4141 0813 28 | ØD 25.4 mm (1"). Order together with 4141 0806 28. Suitable for concentric collet MINI and REGULAR.
4141 0813 29 | ØD 26 mm. Order together with 4141 0806 28 or 4141 0807 28 or 4141 0676 04. Suitable for concentric collet MINI and REGULAR.
4141 0814 08 | ØD 28.58 mm. Order together with 4141 0810 03. Suitable for concentric collet HD.
4141 0814 09 | ØD 29 mm. Order together with 4141 0809 09. Suitable for concentric collet HD.
4141 0814 10 | ØD 29.4 mm. Order together with 4141 0809 10. Suitable for concentric collet HD.
4141 0814 11 | ØD 29.8 mm. Order together with 4141 0809 11. Suitable for concentric collet HD.
4141 0814 16 | ØD 31.75 mm (1 1/4"). Order together with 4141 0810 04. Suitable for concentric collet HD.
4141 0814 17 | ØD 32.15 mm. Order together with 4141 0809 17. Suitable for concentric collet HD.
4141 0814 24 | ØD 34.93 mm. Order together with 4141 0810 05. Suitable for concentric collet HD.