# Mandrel

Ordering No. | Type | Remark
--- | --- | ---
4141 0806 05 | A | Ød 9.2 mm. Order together with 4141 0813 05. Suitable for concentric collet MINI and REGULAR.
4141 0806 08 | A | Ød 10.2 mm. Order together with 4141 0813 08. Suitable for concentric collet MINI and REGULAR.
4141 0806 09 | A | Ød 10.5 mm. Order together with 4141 0813 09. Suitable for concentric collet MINI and REGULAR.
4141 0806 10 | A | Ød 10.9 mm. Order together with 4141 0813 10. Suitable for concentric collet MINI and REGULAR.
4141 0806 11 | A | Ød 11.25 mm. Order together with 4141 0813 11. Suitable for concentric collet MINI and REGULAR.
4141 0806 12 | A | Ød 11.5 mm. Order together with 4141 0813 12. Suitable for concentric collet MINI and REGULAR.
4141 0806 13 | A | Ød 11.9 mm. Order together with 4141 0813 13. Suitable for concentric collet MINI and REGULAR.
4141 0806 14 | A | Ød 12.3 mm. Order together with 4141 0813 14. Suitable for concentric collet MINI and REGULAR.
4141 0806 15 | A | Ød 12.7 mm. Order together with 4141 0813 15. Suitable for concentric collet MINI and REGULAR.
4141 0806 16 | A | Ød 20.6 mm. Order together with 4141 0813 16. Suitable for concentric collet MINI and REGULAR.
4141 0806 18 | A | Ød 13.9 mm. Order together with 4141 0813 18. Suitable for concentric collet MINI and REGULAR.
4141 0806 20 | A | Ød 14.7 mm. Order together with 4141 0813 20. Suitable for concentric collet MINI and REGULAR.
4141 0806 21 | A | Ød 15.1 mm. Order together with 4141 0813 21. Suitable for concentric collet MINI and REGULAR.
4141 0806 22 | A | Ød 15.5 mm. Order together with 4141 0813 22. Suitable for concentric collet MINI and REGULAR.
4141 0806 23 | A | Ød 15.9 mm. Order together with 4141 0813 23. Suitable for concentric collet MINI and REGULAR.
4141 0806 24 | A | Ød 16.3 mm. Order together with 4141 0813 24. Suitable for concentric collet MINI and REGULAR.
4141 0806 26 | A | Ød 17.1 mm. Order together with 4141 0813 26. Suitable for concentric collet MINI and REGULAR.
4141 0806 28 | A | Ød 17.9 mm. Order together with 4141 0813 28. Suitable for concentric collet MINI and REGULAR.
4141 0860 03 | A | Ød 4.14 mm. Order together with 4141 0813 03. Suitable for concentric collet MINI and REGULAR.
4141 0809 09 | A | Ød 21.5 mm. Order together with 4141 0814 09. Suitable for concentric collet HD.
4141 0809 10 | A | Ød 29.4 mm. Order together with 4141 0814 10. Suitable for concentric collet HD.
4141 0809 11 | A | Ød 29.8 mm. Order together with 4141 0814 11. Suitable for concentric collet HD.
4141 0809 16 | A | Ød 31.75 mm (1 1/4" mm). Order together with 4141 0814 16. Suitable for concentric collet HD.
4141 0809 17 | A | Ød 24.6 mm. Order together with 4141 0814 17. Suitable for concentric collet HD.
4141 0676 01 | B | Ød 5 mm. Order together with 4141 0813 01. Suitable for concentric collet MINI and REGULAR.
4141 0676 02 | B | Ød 6.7 mm. Order together with 4141 0813 02. Suitable for concentric collet MINI and REGULAR.
4141 0676 03 | B | Ød 14.7 mm. Order together with 4141 0813 20. Suitable for concentric collet MINI and REGULAR.
4141 0676 04 | B | Ød 17.9 mm. Order together with 4141 0813 28. Suitable for concentric collet MINI and REGULAR.
4141 0676 05 | B | Ød 11.5 mm. Order together with 4141 0813 12. Suitable for concentric collet MINI and REGULAR.
4141 0676 06 | B | Ød 7.5 mm. Order together with 4141 0813 03. Suitable for concentric collet MINI and REGULAR:
4141 0810 03 | B | Ød 21.75 mm. Order together with 4141 0814 08. Suitable for concentric collet HD.
4141 0810 04 | B | Ød 24.25 mm. Order together with 4141 0814 16. Suitable for concentric collet HD.
4141 0810 05 | B | Ød 26.65 mm. Order together with 4141 0814 24. Suitable for concentric collet HD.
4141 0807 01 | C | Ød 5 mm. Order together with 4141 0813 01. Suitable forconcentric collet MINI and REGULAR.
4141 0807 03 | C | Ød 7.6 mm. Order together with 4141 0813 03. Suitable for concentric collet MINI and REGULAR.