# Guía de referencia rápida

To provide a better overview of the system, the following instruction touches upon the steps that are required to start using the system.

The instruction does not cover all system features, but focuses on the most basic.

## Interfaz web

1. Select the type of tool to use. The tightening strategies available, depend on the type of tool you select.

2. Defina un programa de apriete que contenga todos los parámetros importantes de un apriete, por ejemplo el ángulo objetivo y el par objetivo. El objetivo principal de la herramienta es realizar un apriete.

3. Cree una Estación virtual y asígnele una herramienta. La estación virtual actúa como una interfaz entre el controlador y la herramienta y permite conectar varias herramientas a un único controlador físico. Se requiere una estación virtual incluso cuando solo hay una herramienta conectada al controlador.

4. Asignación de una tarea a una estación virtual La tarea puede ser un programa de apriete, una secuencia de grupos o una entrada digital especificada (por ejemplo, un escáner de código de barras). Ahora la herramienta asignada a la estación podrá realizar la tarea.

## Mobil GUI

1. Select the type of tool to use.

2. Create a tightening Task and set the relevant parameters, for example target torque and target angle. El objetivo principal de la herramienta es realizar un apriete.

3. The created task will be assigned to a virtual station. Ahora la herramienta asignada a la estación podrá realizar la tarea.