# Exporting Data from the Mobile GUI

To export data from the mobile interface, do the following:

1. 컨트롤러 탭으로 이동합니다.

2. In the Export menu, tap the Ellipsis icon (...).

3. 옵션 한 개 선택:

   - 모든 컨트롤러 정보

   - 설정 및 구성

   - 연결된 공구로부터의 로그

   - 결과

4. Tap To Device to download the selected data into the mobile device.

5. Tap To USB to download the selected data into a correctly formatted USB storage device connected to the USB port on the front part of the controller.

All controller information and Settings and configurations do not include information about the connected tools.

설정 및 구성 옵션은 설정만 내보내며, 이러한 내보내기는 시간이 별로 걸리지 않습니다.

For STB, SRB, and TBP tools, it is only possible to export logs.

컨트롤러에 연결된 공구가 없을 때 연결된 공구의 기록을 선택해도 파일이 내보내기된다는 점을 참조해 주세요.

컨트롤러에서 조임 결과를 내보내는 데에만 사용함