# Exporting Data from the Mobile GUI

To export data from the mobile interface, do the following:

1. 转到控制器 选项卡。

2. In the Export menu, tap the Ellipsis icon (...).

3. 选择一个选项

   - 所有控制器信息

   - 设置和配置

   - 来自已连接工具的日志

   - 结果

4. Tap To Device to download the selected data into the mobile device.

5. Tap To USB to download the selected data into a correctly formatted USB storage device connected to the USB port on the front part of the controller.

All controller information and Settings and configurations do not include information about the connected tools.

设置和配置选项仅导出相关设置且执行时用时较小。

For STB, SRB, and TBP tools, it is only possible to export logs.

注意：在控制器未连接工具的情况下，当选择“来自连接工具的日志”选项时，仍将导出一个文件。

用于仅从控制器导出拧紧结果