# 使用统计选项卡

Tasks are configured in the Task menu. A task runs a tightening program and can be monitored from the Mobile GUI. The results of the task are presented in the Results menu.

To create a tightening program, create a task and select a strategy, either Tighten to Torque or Tighten to Torque plus Angle.

PF6000 拧紧程序需要设定好参数，以执行拧紧。 Entering a value for Target Torque is mandatory, as well as Target Angle if Tighten to Torque plus Angle was chosen. Other settings are optional, such as Program name, Peak Torque and Angle. 此外，还可以通过添加扭矩或螺母旋转角度必须遵守的限制范围来监控整个拧紧过程。

It is possible to run two types of tightening programs from the Mobile GUI, Tighten to Torque and Tighten to Torque plus Angle.

Multistep programs and other types of tightening programs are available in the Web GUI, and should not be assigned to the Virtual Station 1, to avoid incorrectly displayed results.

此部分内容

- 创建拧紧程序
- 编辑拧紧程序
- 删除拧紧程序