# Technical Data

## Product Data

Maximum Air Pressure | 6.0 bar (87.0 psig)
Maximum Air Consumption | 400 l/min @ 60 screws per minute (HTM & FTM) 800 l/min @ 60 screws per minute (VTM)
Fill Volume | 3.15 l
Screw Size | M3-M6
Screw amount approximately | 1500 (M6 x 25) – 18 000 Screws (M3 x 6)
Weight | 38 kg (84 lb)
Supply Voltage/Frequency | 230 V/50 Hz (EU Version) or 115V/60Hz (US Version)
Rated Power | 25 W
Air Connector | Quick coupling plug KS-4-1/4-A (default) (Changeable to custom specific. Base = G1/4”)

## Applies to: