# Storage

The devices and, if necessary, spare parts should be stored in a packaged condition, which provides further protection against environmental influences.

The following conditions for storage must be observed

- Never store outdoors - not even for a short time

- The components should be stored in a dry place, and should be protected from dust and aggressive media

- Protect from sunlight

- Avoid mechanical vibration

- Storage temperature: + 10 ° C to + 55 ° C. High variations of temperature should be avoided

- Relative humidity: 5% to 95% (not condensing)

- If the device is stored for longer than a month, the condition of all parts and the packaging should be checked regularly, if necessary refresh/renew the preservation

- If possible, the packaging should only be removed immediately before assembly

The packaging may contain further information on transport and storage, this information must be strictly observed.

## Applies to: