# Draining the Condensate Automatically

NOTICE

The Condensate Can Cause Damage to the Compressed Air System

With the automatic condensate drain, the valve opens automatically as soon as the floater has reached the highest point. The valve closes automatically when the floater reaches the lowest point.

To switch to automatic mode, turn the drain screw counterclockwise as far as it goes.

If the screw is screwed in completely, the automatic drainage is blocked.

## Applies to: