# Main Components of the Screw Feeding System

The individual components of the system can be customer specific, and may therefore differ from the components shown here.

The screw fastening system consists of the following main components

No. | Component | Function
1 | Screw Feeding Tightening Module Driving Tool Screw Feeding Front Part | To carry out the screwing process.
2 | Power Focus 6000 | Control and monitoring of the screw fastening and feeding process.
3 | Screw Feeding Unit | Transport, sort and separating the screws, feed the screws into the Screw Feeding Tightening Module using compressed air.
4 | Tool Cable | Electrical connection between the Power Focus 6000 and the Screw Feeding Tightening Module.
5 | Connecting Line | Electrical connection between the trigger on the Screw Feeding Tightening Module and the Screw Feeding Unit.
6 | Air Connection | Pneumatic connection for Forward and Return Stroke between the Screw Feeding Tightening Module and the Screw Feeding Unit.
7 | Connection Cable | Electrical connection between the Power Focus 6000 and the Screw Feeding Unit.
8 | Signal Line | Connection between the Power Focus 6000 and the Screw Feeding Unit.
9 | Feeding Tube | Pneumatic transport of screws from the Screw Feeding Unit to the Screw Feeding Tightening Module.

For more information about the Screw Feeding Tightening Module, see product information for the Screw Feeding Tightening Module.

For more information about the Power Focus 6000, see product information for the Power Focus 6000.

In this Section

- Components and Function of the Screw Feeding Unit
- Screw Container
- Step Conveyor Unit and Linear Guide
- Separating Unit
- Overview of Electrical and Pneumatic Components
- Feeding Tube
- Controls
- Functional Description of the Screw Feeding Unit

## Applies to: