# Maintenance Instructions

WARNING

Electrical Hazard

Risk of electric shock.

- Always disconnect the machine and equipment from all power sources before carrying out any maintenance or repair.

WARNING

Cutting Hazard

Sharp objects can cause injuries, especially to the hands.

- Always wear cut resistant gloves when changing components, making repairs or removing a blockage.

WARNING

Risk of severe injury

Air under pressure can cause injury.

- Always shut off the air supply when not in use or before any adjustments.

- Drain the hose of air pressure and disconnect the tool from air supply when not in use or before any adjustments.

- Always use the correct hose size and air pressure for the tool.

Only Atlas Copco Industrial Technique AB original fuses with the specified amperage may be used, if they need to be replaced.

In this Section

- Draining the Condensate Automatically
- Draining the Condensate Manually
- Emptying and Cleaning the Collection Containers
- Replacing the Feeding Tube

## Applies to: