# Getting Started

To access I/O Hub Settings, contact your local Atlas Copco Service Technician or Sales Representative.

The default password for I/O Hub Settings is password.

1. Open I/O Hub Settings on the computer connected to the I/O Hub 8-PS. Connection between I/O Hub 8-PS and computer can be either direct or via a controller.

2. In the I/O Hub Settings home menu, select Search.

   Make sure that the IP address of the I/O Hub 8-PS and the IP address of the computer network adapter are in the same IP range.

3. Set the IP address for the I/O Hub 8-PS either manually or via DHCP server.

4. Open the I/O Hub Web Interface and set the IP address for the controller.

It is also possible to access the I/O Hub Web Interface by searching for the device IP address in a web browser (I/O Hub IP address/hmi.html Ex: http://169.254.1.254/hmi.html).

Relevant Information

- Setting the Controller IP Address
- Setting the I/O Hub IP Address