# Performing Network Reset

The I/O Hub 8-PS can be reverted back to its network related original default settings.

To prevent the ARGEE program from being deleted when the device is reset, make sure that the program is locked.

1. In the I/O Hub Settings home menu, select Search.

2. Select the required device or devices.

3. Select Actions > Network reset.

4. A dialog box will appear. Confirm the reset by selecting Yes.

5. Wait 5 seconds before selecting Search in the I/O Hub Settings home menu.

Relevant Information

- Locking and Unlocking the ARGEE Program