# Updating the ARGEE Program

When ARGEE program is updated, I/O Hub Web Interface will also be updated.

Make sure that the ARGEE program is not locked.

Make sure that the IP address of the I/O Hub 8-PS and the IP address of the computer network adapter are in the same IP range.

1. In the I/O Hub Settings home menu, select the required device or devices.

2. Select ARGEE > Load program.

3. Select the Override existing programs checkbox.

4. Select Open and find the location where the ARGEE programs are stored on your computer. Select the program.

5. Select Start. When download is completed, the message Program download successfully completed appears in the Status message column.

6. Select Close.

7. Wait 5 seconds before selecting Search in the I/O Hub Settings home menu. The new ARGEE program is now displayed in the ARGEE column.

Relevant Information

- Locking and Unlocking the ARGEE Program