# Setting the I/O Hub IP Address

The factory set IP address is 169.251.1.1.

1. In the I/O Hub Settings home menu, select Search.

2. Select the required device.

3. Select Change and change the IP address and, if required, the network mask and gateway.

4. Select Set in device to save. The new IP address is now displayed in the IP address column.

Make sure that IP address of the I/O Hub 8-PS and the IP address of the computer network adapter are in the same IP range.