# Working with the Tools and Status Screens

## The Tools screen

The Tools screen shows an overview of all connected tools. The status of each virtual station is indicated with different colors.

Color | Status
--- | ---
Green | Tool unlocked
Blue | Tool locked
White | Power Focus not connected
Gray | ILT Tool Tag not connected

## Activating the Tools screen

- Select Status to access the Tools screen from the Home screen.

## The Status screen

From the Tools screen it is possible to access the Status screen for each virtual station. The Status screen displays which area and tightening program that are active and whether the tool is enabled or disabled. It also shows current measurements for orientation and distance.

An open padlock symbol shows that an Area is enabled.

A closed padlock symbol shows that an Area is disabled.

Only one area can be active at the time.

## Viewing a specific Area on the Status screen

- Select the configuration symbol and select an Area from the list to view it in detail.

## Activating the Status screen

- On the Home screen, select Status, and select a Virtual Station on the Tools screen. The Status screen opens.

The Status screen will also be displayed after the Inactivity Timeout has been reached if one tool is used. If multiple tools are used the Tools screen will be displayed.

## Changing font size on the Status screen

- On the Status screen, select the symbol with the small and large T to switch between font sizes. The small font size is default.

Relevant Information

- Setting the Inactivity Timeout