# Rundown Stage

The part of the tightening from when the screw enters the thread until just before the screw head touches the underlying surface and snug is reached. The torque required during rundown does not contribute to any clamping force.

Parameter | Description | Default value
--- | --- | ---
Rundown speed | Defines the speed during the Rundown step | Tool max speed

In this Section

- Selftap
- Rundown Torque Limits
- Rundown Angle Limits
- Post View Torque
- Rundown Complete