# Batch Completed - 30

Batch Completed is an output signal which is triggered when the batch is complete.
The batch result status (OK or NOK) has no effect on the Batch Completed signal.

Name in SoftPLC: BATCH_COMPLETED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE