# Running the External Result Tightening Strategy with a Tool Connected

1. On the Home view, select the Tightening Tab. Then, create a tightening program with External Result strategy.

2. Return to the Home view and select the Virtual Station Tab.

   In the Licenses window, the External Result Tightening Strategy with a Tool Connected feature requires a license to be assigned and used by a virtual station.

3. In the Tool window, select the necessary tool. Then, select the tool configuration.

4. In the Task window, select the tightening program with an External Result strategy.

5. Send EXTERNAL_OK signal to the Virtual Station.

6. Select Go Result button to display the results.
   Results are sent from the Tool configuration for the tool connected to the Virtual Station.

Relevant Information

- Assigning Licenses to a Virtual Station
- Connecting a Tool to a Virtual Station