# Direction

Direction defines the tightening direction of the spindle to clockwise (CW) or counterclockwise (CCW). The rotation of the spindle will always be in this direction, except when loosening and during the conditioning step used in the Three step strategy.

Parameter | Description | Default value
--- | --- | ---
Thread direction | Defines the tightening direction of the spindle. | Clockwise