# Turn on the system

When turning on the system the power residual current device may switch off the power.

Before you power up the system make sure it is installed the same way as it was planned and configured. Otherwise it will not work.

1. On the FlexCarriers, switch the circuit breakers on (up).

2. Fasten the FlexCarrier cover. Use torque 2.2 Nm.

   Make sure the cables are not pinched or damaged when the cover is put back on.

   Do not draw the cables in the way of the LED light guide in the cover.

3. Turn the handle on the mains switch box. This will turn the system on.

The FlexSystem is now potentially dangerous since the e-stop functionality is not tested yet.