# Result View - Numbers

The first window will display the result in numbers.

1 | Virtual station name
2 | Batch sequence name
3 | Batches in sequence An OK batch is colored green. An ongoing batch is colored yellow. An NOK batch is colored red.
4 | Tightenings in batch An OK tightening is colored green. An ongoing tightening is colored yellow. An NOK tightening is colored red.
5 | Result status An NOK tightening will give a detailed status of the unsuccessful tightening.
6 | Target torque/angle
7 | Tightening program name
8 | Number of completed batches in sequence
9 | Number of completed tightenings in a batch
10 | Tightening result