# Balancers

The Screw Feeding System can be extended with balancers for weight compensation and positioning.

## Spring Balancer RIL

The RIL weight compensators always keep the tool within reach. RIL weight balancers are supplied with tension adjustment. A safety chain is supplied with all RIL balancers.

For more information on the available RIL balancers, refer to the product page of the specific model:

Spring Balancer RIL | Product Number | Type
--- | --- | ---
RIL 2C | 8202 0701 19 | Standard
RIL 4C | 8202 0702 18 | Standard
RIL 5C | 8202 0703 25 | Standard
RIL 10C | 8202 0704 16 | Standard
RIL 10CS | 8202 0704 20 | Balancer equipped with automatic safety drum lock in case of spring failure.

## Spring Balancer WP

The WP balancers enable the simplest positioning. The conical rope drum keeps the suspended load in suspension over the entire extension length of the rope, and makes it weight-free for the operator. The housings of the WP 05/10 balancers are made of plastic, while those of the WP 20 and WP 30 series are made of aluminum. All models (except WP 20) have a swiveling safety suspension hook.

For more information on the available WP balancers, refer to the product page of the specific model:

Spring Balancer WP | Product Number | Type
--- | --- | ---
WP 05-3 | 8202 0778 01 | Standard
WP 05-4 | 8202 0778 02 | Standard
WP 05-3-A | 8202 0778 06 | Extended cable - A
WP 05-4-A | 8202 0778 07 | Extended cable - A