# Reading a Tightening Result

The tightening result is presented graphically with a result gauge. The gauge is divided into three parts indicating either an OK or NOK tightening. Field colors (red for NOK, green for OK) are only shown at tightening result.

Position | Name | Description
--- | --- | ---
1 | Final torque or final angle | Torque/angle when tightening program has concluded.
2 | Target torque or target angle | Torque/angle which was aimed for.
3 | Min limit | Indicates lower limit of OK tightening (min angle or min torque)
4 | Indicator | Gauge indicator showing the result on the scale
5 | Low field | Indicates NOK tightening due to low angle/torque
6 | Tightening program | Sequence number and name of the tightening program used
7 | OK field | Indicates an OK tightening
8 | Max limit | Indicates upper limit of OK tightening (max angle or max torque)
9 | Hi field | Indicates NOK tightening due to high angle/torque