# Cable Information

## Power Cable

- Power cable with standard raw cable, M12 4 pin open wires

- Connector: female 4 pin M12 A-coded

Pin Assignment
Side A Pin Nr | Wire Color | Side B Pin Nr | Function
--- | --- | --- | ---
1 | White | Open wire | +24V
2 | Yellow | Open wire | +24V
3 | Brown | Open wire | GND
4 | Green | Open wire | GND

## Ethernet Cable

- Standard Ethernet cable, M12 x-coded for PoE+

Pin Assignment
Side A M12 x-coded Pin Nr | Wire Color | Side B RJ-45 Pin Nr
--- | --- | ---
1 | Orange-white | 1
2 | Orange | 2
3 | Green-white | 3
4 | Green | 6
7 | Blue-white | 5
8 | Blue | 4
5 | Brown-white | 7
6 | Brown | 8

## Applies to:

8436 6771 00
8436 6771 01