# Additional Maintainance Safety Messages

WARNING

Moving parts Hazard - Loose Tubes

Unexpected pneumatic movements of loose tubes cause high outflows of compressed air. This may lead to severe injuries especially to the eyes.

- Always make sure that there are no damages or loose hoses or fittings.

- Always shut off the air supply, drain hose of air pressure, and disconnect tool from air supply when not in use, before changing accessories or when making repairs.

- Never direct air at yourself or anyone else.

- Whenever universal twist couplings are used, lock pins must be installed.

- Do not exceed maximum air pressure of 5 bar / 73 psi, or as stated on the tool name plate.

WARNING

Moving parts Hazard – Feeding Tubes

Unexpected pneumatic movements of the feeding tubes cause outflows of screws at high speed. This may lead to severe injuries especially to the eyes.

- Always verify that all connections between the Feeding Tube and the Swivel Arm are securely fastened before pressurizing the tool.

  The pneumatic power supply must be switched off and vented during all work on the Screw Feeding Tightening Module.

  Always make sure that there are no damages or loose feeding tubes or fittings.

  Always shut off the air supply, drain hose of air pressure, and disconnect tool from air supply when not in use, before changing accessories or when making repairs.

  Never direct air at yourself or anyone else.

  Whenever universal twist couplings are used, lock pins must be installed.

WARNING

High Pressure Hazard

Due to damaged or inadequately inserted compressed air hoses into the couplings, air can escape under high pressure and may cause injury to the eyes.

- Regularly check the feeding tubes for damage.

- In the case of damage to the pneumatic components, the system must be switched off immediately, de-aerated and secured against being switched on again. And, proceed to repair.

NOTICE

Disposal of System Components

Incorrect disposal of the system components leads to contamination of the environment.

- The components of the system must be disposed of via designated collection facilities appointed by government or local authorities.

- For more information about disposal of your old product, please contact your city office, waste disposal service, or your Atlas Copco representative.

## Applies to: