# Viewing and filtering the event log

You must first navigate to Smart AMS Manager.

- Go to the Smart AMS Manager address in your web browser by using the Open Smart AMS Manager shortcut on the Desktop or on the Windows Start menu.
  Sample address: http://localhost:6394. Port number is selected when you install Smart AMS. The default is 6394. Make sure to replace localhost with the actual IP address of the computer that Smart AMS Manager is running on.

- To switch to the Event Log section, click in the Navigation Panel on the left of the page. On mobile devices with a smaller screen, click your username in the upper right corner of the page, and then select Event Log.

- To get the latest data, click Refresh.

Logs include the following information about events: time, origin, level, event type, alarm (On or Off), message, and details.

## Services event history

In the Services Event History subsection you can find entries for events, including disconnections between Smart AMS and the server, disconnections between tools and controllers (with reference to the station), disconnections between the server and PLC, errors occurred during production, product sign-in and sign-out operations, changing of product status.

You can filter records by time stamp, source type, event type, message text, log level, and alarm.

1. Click the column header.

2. Specify the filter condition.
   The column header will be displayed in bold italic type.

   You can use an asterisk (*) in the filter to match any number of characters, where applicable.

3. Click Refresh.

To remove a filter, click the column header, and then delete any text from the Filter box. Alternatively, click Reset to revert to the default view.

To configure the advanced filters:

1. Click the Advanced filters wording.

2. In the Level list, select the log level of your choice: All, Info, Warning, Error, or Fatal.

3. In the Alarm list, select On, Off, or No Alarm Indication. You can combine these.

- To change the number of entries that are displayed on each page, click the drop-down list under the results table, and then select 5 rows, 10 rows, 20 rows, 25 rows, 50 rows, 100 rows, or 500 rows.

- To navigate between pages, use the page navigation buttons (Previous, Next) available on pages. The total number of pages is shown on each page.

- To jump quickly to a page, enter a page number in the Page box.

To view event details:

1. Click in the DETAILS column, if available. Event details are displayed in the JSON format.

2. To close the details popup, click a second time.

## Manager event history

In the Manager Event History subsection you can find entries for events pertaining to Smart AMS Manager. Example: a service is successfully started or stopped.

## Applies to: