# Tool Configuration

On the home view, go to the Configurations tab and select Tool Configuration on the left pane to configure the available accessory functions on the tool.

Different functions are available depending on the tool type.

## Configuring Accessory Functions on the Tool

1. On the Configuration window, select Filter by tool type. Then, select the relevant tool.

2. On the Configuration window, select Edit to configure the relevant functions.

   A configuration assigned to a virtual station cannot be deleted.

3. If available, configure the Function Button, the LED Ring, the Direction Switch, the Buzzer and the Vibrator by selecting the ellipsis icon on the corresponding fields.
   Each field shows a number which corresponds to the number of the specific function (for example, 1 corresponds to Function Button, 2 to LED Ring, 3 to Direction Switch, 4 to Buzzer and 5 to Vibrator).

4. If available, configure the General Settings, the Start condition and the Accessory Bus on its corresponding windows according to the customer needs.

In this Section

- Configuration of the Function Button
- Configuration of the Tool LEDs
- Configurtion of the Direction Switch
- Configuration of the Buzzer
- General Settings
- Configuration of the Start Condition
- Configuration of the Accessory Bus
- Configuration of the Open End