# Cable Matrix

Refer the below matrix for different cable combinations to connect CAN converter

Accessory Abbreviations used in the table

IB | Indicator Box
IO | IO Expander
SL | Stack Light
OP | Operator Panel

Cable matrix for PF6 FlexSystem
PF6 FlexSystem | CAN converter | M23 to CAN | M12 to IO | CAN Splitter | CAN
Compatible |  |  |  |  |
SL | X |  |  |  |
SL+OP | X |  |  |  | X
SL+IO | X |  |  |  | X
SL+IB | X | X | X |  | X
SL+OP+IO | X |  |  |  | 2X
SL+OP+IB | X | X | X | X | 2X
SL+IO+IB | X | X | X |  | 2X
SL+OP+IO+IB | X | X | X | X | 2X
OP | X |  |  |  |
OP+IO | X |  |  |  | X
OP+IB | X | X | X |  | X
OP+IO+IB | X | X | X | X | X
IO | X |  |  |  |
IO+IB | X | X | X |  | X
IB | X |  |  |  |

Cable matrix for IxB - TC
IxB - TC | CAN converter | M23 to CAN | M12 to IO | CAN Splitter | CAN
SL | X |  |  |  |
SL+OP | X |  |  |  | X
SL+IO | X |  |  |  | X
SL+S4/6 | X |  |  |  | X
SL+OP+IO | X |  |  |  | 2X
SL+OP+S4/6 | X |  |  |  | 2X
SL+IO+S4/6 | X |  |  |  | 2X
SL+OP+IO+S4/6 | X |  |  |  | 3X
OP | X |  |  |  |
OP+S4/6 | X |  |  |  | X
OP+S4/6 | X |  |  |  | X
OP+IO+S4/6 | X |  |  |  | 2X
IO | X |  |  |  |
IO+S4/6 | X |  |  |  | X
S4/6 | X |  |  |  |

Cable matrix for PF IRC
PF IRC | CAN converter | M23 to CAN | M12 to CAN | M12 to IO | CAN
SL | X |  |  |  |
SL +OP | X |  |  |  | X
SL+IO | X |  |  |  | X
SL+S4/6 | X |  |  |  | X
SL+OP+IO | X |  |  |  | 2X
SL+OP+S4/6 | X |  |  |  | 2X
SL+IO+S4/6 | X |  |  |  | 2X
SL+IO+OP+S4/6 | X |  |  |  | 3X
OP | X |  |  |  |
OP+S4/6 | X |  |  |  | X
OP+S4/6 | X |  |  |  | X
OP+IO+S4/6 | X |  |  |  | 2X
IO | X |  |  |  |
IO+S4/6 | X |  |  |  | X
S4/6 | X |  |  |  |