# Set-up for Accessories

Compatible accessories for the CAN converter:

- Stack Light

- Operator Panel

- Indicator Box

- Socket Selector

- IO Expander

It is possible to daisy chain up to 5 accessories to the CAN converter. Connect the accessories to the CAN Converter with CAN cables. An example setup is shown in the image below:

1 | Indicator Box
2 | IO Expander
3 | Socket Selector
4 | Stack Light
5 | Operator Panel

The Operator Panel only has one CAN connection. If it is not the last or only accessory in the daisy chain a CAN splitter(Y-Cable) is needed. For example, a daisy chain with an indicator box

It is possible to add additional power to the daisy chain if needed:

- Add extra power to the accessories in the daisy chain. The power is supporting the accessory which it is connected to.

- Connect an I/O Hub PSU (product number 4390208153) to the daisy chain

If the socket selector is the first or only accessory in the daisy chain, a extension cable(Male to Female D-sub) should be used to connect CAN converter and Socket selector. Example set up is shown in the image below

In this Section

- Accessories Matrix
- Cable Matrix