# Ambient Temperature

For best battery performance and life time, keep battery within temperature intervals.

Operating temperature, charge | +5 to +40 °C (+41 to +104 °F)
Operating temperature, discharge | 0 to +40 °C (+32 to +104 °F)
Transportation temperature | −20 to +40 °C (−4 to +104 °F)
Storage temperature | +10 to +25 °C (+50 to +77 °F)

Do not place battery in direct sunlight.

## Applies to: