# Checking the Drive Direction

Before you use the wrench, make sure that the direction of rotation is correct. The direction is indicated by the arrow on top of the tool.

The reaction arm will rotate in the opposite direction to the drive until it contacts a suitable reaction point.

1 | Loosen: counterclockwise Tighten: clockwise
2 | Reaction arm
3 | Direction arrow

If the direction of rotation needs to be reversed, turn the wrench over and install it on the application.

## Applies to: