# Test run

- Enable transducer from minload: when the checkbox is unselected, the transducers whose minimum operating range value is lower than the inspection minimum torque value can be used to run the test.
  When the checkbox is selected, the transducers whose minimum load value is lower than the inspection minimum torque value can be used to run the test.
  By default, the Enable transducer from minload checkbox is disabled.

NOTICE

The accuracy of the measurements is guaranteed only within the declared transducer operating range.

## Applies to: