# Pairing IRC-Connect

1. In the Toolbar, tap Measuring devices.

2. On the upper-right corner of the Measuring devices page, tap Add ().

3. In the Measuring devices type window, tap IRC-Connect.

   After selecting IRC-Connect in the Measuring device type window, the Connection category is automatically displayed.

   The General category is automatically complete after the pairing process.

4. In the Connection category, configure the following parameters:

   - Connection type: select IRC-B.

   - Trace read: select one of the following option for the trace reading from the IRC-Connect:

     - Always: the traces are always read.

     - NOK only: only NOK traces are read.

     - Never: the traces are never read.

   - Gyro compensation: select the check box to enable the gyro compensation.

5. On the IRC-Connect, press the power switch for five times: the Radio LED is lit steady, and the Result LEDs start blinking in sequence.

6. On the upper-right corner of the Toolbar on the STpalm, in the Add IRC-Connect page, tap the More option icon (). Then, tap > Pair.

   The Pairing instructions dialog box opens.

7. Turn on the IRC-Connect clicking the power button placed on the main panel:

   A | Main panel | B | Result LEDs
   C | Radio LED | D | Power button

8. After IRC-Connect boot sequence is completed, press five times the IRC-Connect Power button.

9. After two seconds the Radio LED is lit steady and the Result LEDs start blinking in sequence.

10. The IRC-Connect is now in pair mode. On the lower-right corner of the Pairing instructions dialog box on the STpalm, tap Pair.

11. At the end of the pairing process, on the Pairing window, tap OK .

    In the Add IRC-Connect page, the General section is automatically displayed with the following parameters:

    - Name: name of the paired measuring device.

    - Serial number: serial number of the paired measuring device.

    - Firmware version: firmware version of the paired measuring device.

    - Notes: type optional notes.

12. On the upper-right corner of the Add IRC-Connect page, tap Save.

## Applies to: