# Stored Results View

The tool stores the result for every tightening or loosening performed.

View stored results

1. Go to Reports in the home menu and select Results in the left pane.

2. Select View all results. The result list will show information about:

   - Date: date and time of the tightening performed.

   - Tightening Program: Tightening Program column shows Multistep Tightening Program name, or Batch Sequence name followed by the Tightening Program name within the Batch Sequence.

   - Result: Torque / Angle result.

   - Limits: Limits column shows only when the user sets Step Monitor or Step Restriction (Step level), or Program Monitor or Program Restrictions (Multistep Program level).

     Step Monitors, Step Restrictions, Program Monitors and Program Restrictions are applicable for Final Torque and Final Angle.

   - Details: Tightening / loosening result details.

   - Trace checkbox: By selecting a trace checkbox the corresponding result will be shown in the Sync Trace Result View.

   Results marked with a red bar have status NOK. For descriptions of NOK results, see the NOK Result List.

3. Select a result in the list to enter the Trace Result View.
   The Trace Result View window shows, step by step, the tightening life-cycle.
   When the tightening is NOK, the Trace Result View shows which Step Monitor or Step Restriction that caused it.

On the upper-right corner of the trace graph, select the left-arrow / right-arrow to show the necessary trace graph.
The following trace graphs are available:

- Torque / Time

- Torque / Angle

- Angle / Time

On the trace graph, it is possible to zoom in/out, move the trace, and read x-axis and y-axis values on a specific point.
On the lower-left corner of the trace graph, select "+" to zoom in , "-" to zoom out, or the "square icon" to reset the zoom level back to the default view.

On the lower part of the Trace Result View window, detailed step information is shown.

In this Section

- Viewing Synchronized Traces