# Creating a Tightening Program

1. Go to Tightening in the home menu.

2. Select the plus icon.

3. In the Choose Operation Mode window, select Tightening.

4. Open the Properties window and type in a valid Maximum Torque Limit for the specific tool. Type Enter. Close the Properties window.

5. Open the Steps pane on the right and drag and drop the steps to create a tightening program.

6. Set Monitors and Restrictions for each step as applicable and press the Enter key.