# From SoftPLC - 10064

Allocated bytes for data transfer from PLC to accessories.

Name in SoftPLC: FROM_PLC

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | uint8 array | 8 | 8

## Devices

- Filedbus: FALSE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE