# Target/Final Torque - 30101

Signal displaying the target/final torque alternatively.

Target/Final torque is between the target torque and the final torque if a selected tightening program is updated or a new tightening program is selected.

Set Step Category of the last step to Final. The ST Selector displays Target Torque only if the last step has a torque target.

Name in SoftPLC: STSELECTOR_TARGET_FINAL_TORQUE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Integer | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE