# Viewing Tool Information

1. On the sidebar menu, select Integrated Controller Tool .

2. On the top bar of the Integrated Controller Tool page, select the Tool tab.

The Tool category lists the following information on the measuring device:

Information | Description
--- | ---
Model | Measuring device model denomination.
Serial Number | Measuring device serial number. It may be needed for the correct spare parts list or for service instructions.
Product Number | Measuring device product number.

The smartHEAd category lists the following information on the smartHEAD:

Information | Description
--- | ---
Model | smartHEAD model denomination.
Serial Number | smartHEAD serial number. It may be needed for the correct spare parts list or for service instructions.
Maximum Torque | smartHEAD torque capacity.
Product Number | smartHEAD product number.

Tap TAG to view the following information on the TAG:

Information | Description
--- | ---
TAG ID | TAG number.
Torque Correction Coefficient | Torque correction coefficient defined for the TAG.
Angle correction | Angle correction defined for the TAG.
Nominal torque | Torque at which the Angle correction is defined.

The Maintenance category lists the following information on the transducer:

Information | Description
--- | ---
Is transducer overloaded? | Yes - the transducer has been overloaded. No - the transducer has not been overloaded.
Highest torque value | Highest torque output measured by the transducer.
Highest torque date | Date and time when the highest torque output was measured by the transducer.
Angle correction | Angle correction coefficient for the smartHEAD due to the wrench bending. Note that this coefficient is related to the torsion of the smartHEAD itself. When a wrench extension is used, its angle correction coefficient must be calculated and added to the end fitting tool or program parameters. For further information, refer to How to Calculate the Angle Correction.
Transducer calibration date (CW) | Date of the last torque calibration in clockwise direction.
Gyro calibration date (CW) | Date of the last gyroscope calibration in clockwise direction.
Transducer calibration date (CCW) | Date of the last torque calibration in counterclockwise direction.
Gyro calibration date (CCW) | Date of the last gyroscope calibration in counterclockwise direction.
Next calibration date | Date of the next calibration expiration.
Number of measurements | Number of measurements performed by the transducer so far.