# Saving a Configuration

This saves the configuration of all devices currently visible in ILM Manager, meaning that one file for each UWB channel is required.

1. In the upper left corner of the ILM Manager, select the Save icon.
   Save As pop-up window opens.

2. In the Save As pop-up window, navigate to a location to save the configuration.

3. In the File name box, enter a name for the configuration.

4. Select Save.
   An XML-file with the configuration for all ILM devices shown in the Configuration view is created.