# Resetting Movement Detection

1. In the Configuration view, on the Anchors tab, select the ILM Anchor, then select Edit.
   Anchor Details pop-up window opens.

2. In the Anchor Details window, on the Extended tab, clear the Movement Detected checkbox.

3. Close the Anchor Details window.

4. In the Configuration view, select Upload Configuration.
   The status LED of the ILM Anchor will change from red to the color of the configured mode.