# Charging LED Indicators

The MTRwrench 85 indicators, when the wrench is in the cradle and after the zeroing process has been completed, show the operator the status of the charging:

1 led blinking white |  | Battery charging from 0% to 30%
1 led steady white and 2nd blinking white |  | Battery charging from 31% to 60%
2 led steady white and 3rd blinking white |  | Battery charging form 61% to 90%
3 led steady white |  | Battery charging from 91% to 100%