# Tool Health

The Health view includes Temperature entry, which shows information of tool temperature.

## Tool temperature

Tool temperatures (both for cabled and battery tools) are monitored continuously by the POWER FOCUS 6000. Supported temperature units are degrees Celsius (°C) and degrees Fahrenheit (°F), with Celsius as the default unit. It is possible to switch between the two units without requiring a controller restart. When a critical component temperature exceeds the maximum temperature, the tool is locked and an alert (2014) is shown. The tool is once again unlocked when the critical component temperature drops below the temperature limit.

Tool temperature is not available for the STwrench.

## Monitoring Tool Temperature

1. On the Home view, tap on the Tool Tab.

2. Select the Health view, to see the temperature of the various components is displayed.

3. Select the Peak Temperature view to see the list of highest temperatures peaks for each component.

4. Select the Real time temperature view to continuously monitor the temperature of a component.