# Unlock Loosening on Disable - 10150

Used to enable loosenings for a tool that has been disabled due to the Tightening setting Disable loosening in the General Virtual station configuration.

Name in SoftPLC: UNLOCK_LOOSENING_ON_DISABLE

Signal type | Value type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE