# Rundown Complete

Rundown complete sets if the screw has reached snug. It ends the Rundown step so that the tightening step can be entered.

Parameter | Description | Default value
--- | --- | ---
Rundown complete | Specifies how to control when snug is reached. At torque: Specifies the torque value for when the rundown step is completed. | At torque
<At torque> | Defines the torque value for when snug is reached and the rundown step is completed. Rundown complete must be smaller than First torque in multi-step strategies or Target torque in the TurboTight strategy. |