# CRh - Clutch Rehit

Tools
XCB

If the tool clutch is released while the tightening is still within the angle window, the step restriction is triggered. This stops the tightening immediately and produces a NOK result. This step restriction is only valid for the Tighten to Clutch tightening step.

Parameter | Description
--- | ---
Angle Window | The angle window (in degrees) during which the Clutch Rehit step restriction is triggered.