# Waiting To Continue

If in a Wait tightening step with the condition Signal configured as Wait Type, through the sub-signal Waiting To Continue, each individual bolt shows if the related status is waiting for an input to continue.

For more information, see the output signal Waiting To Continue - 201.

Name in SoftPLC: CYCLE_STATUS_WAITING_FOR_CONTINUE

Value Type | Start bit | Length | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Boolean | 7 | 1 | 1 | 1