# Configuring the Remote Logging Connection

To connect a controller to a remote logging server, configure and activate the remote logging settings on the controller.

1. On the home view, go to the Settings tab and select Server connections on the left pane.

2. On the Remote Logging window, configure the following parameters:

Field | Description
--- | ---
On/Off | Enables/Disables communication with the remote logging server
TCP/UDP | Selects TCP or UDP protocol
Server host | Remote logging server IP address
Server port | Remote logging server port

## Configure Log Levels

To configure the logs that are stored on the remote logging server:

1. On the home view, go to the Settings tab and select Server connections on the left pane.

2. On the Remote Logging window, select Configure.

3. On the Configure Facilities window, select the applicable checkboxes.

   Category | SysLog classification
   --- | ---
   Error | Alert, Critical, Emergency, Error
   Warning | Warning
   Info | Informational, Notice

   To restore the selection to the previous configuration, select UNDO.

4. Select Apply.