# Quick Step

Quick step is a tightening strategy used to reduce the joint’s preload scatter by adding an initial step with a given torque and speed, and then reducing the target speed in the final step.

Parameter | Description | Default value
--- | --- | ---
First torque | Target torque for the first step. |
First torque | Torque during first step. | 80% of Target Torque
First speed | Target speed for the first step. |
First speed | Tool speed during first step. | 50% of Tool max speed